[80] CONFIGURATION DIAGRAMS - - TAILGATE | PRINT PAGE / INDEX / PRIOR / NEXT

TAILGATE
F-01 | (1) | Rear window defogger (-)
F-02 | (4) | Rear wiper motor
F-03 | (2) | High-mounted stop lamp
F-04 | (1-B) | Rear window defogger (+)
F-05 | (10) | Floor wiring harness (LH) and tailgate wiring harness combination <LHD> or floor wiring harness (RH) and tailgate wiring harness combination <RHD>
F-06 | (6-B) | Tailgate lock actuator
F-07 | (1-B) | Tailgate switch
F-08 | (2-GR) | Licence plate lamp (RH) <Except 4G63>
F-09 | (4-GR) | Floor wiring harness (LH) and rear bumper wiring harness combination <Except for Hong Kong spec.>
F-10 | (2-GR) | Licence plate lamp (LH) <Except 4G63>
F-11 | (2-B) | No connection
F-12 | (2-B) | Rear fog lamp <Vehicles for Argentina and Hong Kong spec.>

[80] CONFIGURATION DIAGRAMS - - TAILGATE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation