[51] EXTERIOR - - WINDSHIELD WIPER AND WASHER - WINDSHIELD WASHER - REMOVAL AND INSTALLATION <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <2400>
|  |  | Windshield washer nozzle removal steps
--- | --- | --- | ---
|  | • | Connection of windshield washer hose
|  | 1. | Windshield washer nozzle
|  |  | Washer hose removal steps
|  | 2. | Front splash shield (LH) mounting clip
|  | • | Connection of windshield washer nozzle
|  | 3. | Windshield washer hose
|  |  | Washer tank removal steps
|  | • | Front under cover (RH) (Refer to ).
|  | 2. | Front splash shield (RH) mounting clip
|  | • | Connection of front washer hose and rear washer hose
|  | 4. | Washer tank assembly
|  | 5. | Windshield washer motor
|  | • | Headlamp washer motor (Refer to ).
|  | 6. | Rear washer motor
|  | 7. | Washer tank
|  |  | Washer motor removal steps
|  | • | Front under cover (LH) (Refer to ).
|  | • | Connection of front washer hose and rear washer hose
|  | 5. | Windshield washer motor
|  | 6. | Rear washer motor
NOTE: For removal and installation of the wiper and washer switch, refer to GROUP 54A, Column switch .

[51] EXTERIOR - - WINDSHIELD WIPER AND WASHER - WINDSHIELD WASHER - REMOVAL AND INSTALLATION <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation