[35A] BASIC BRAKE SYSTEM - - ON-VEHICLE SERVICE - BRAKE DRUM INSIDE DIAMETER CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| BRAKE DRUM INSIDE DIAMETER CHECK Remove the brake drum.
| Measure the inside diameter of the brake drum at two or more locations. Standard value: 228.6 mm Limit: 230.6 mm Replace the brake drums, shoe and lining assembly when wear exceeds the limit value or is badly imbalanced.

[35A] BASIC BRAKE SYSTEM - - ON-VEHICLE SERVICE - BRAKE DRUM INSIDE DIAMETER CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation