[52A] INTERIOR - - INSIDE REAR VIEW MIRROR | PRINT PAGE / INDEX / PRIOR / NEXT

INSIDE REAR VIEW MIRROR
| REMOVAL SERVICE POINT
| Disengage the claw A and lower the cover toward arrow 1 direction. Push the claw B toward arrow 2 direction to unlock, and pull out the mirror toward arrow 3 direction.

[52A] INTERIOR - - INSIDE REAR VIEW MIRROR | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation