[34] REAR SUSPENSION - - REAR SUSPENSION CROSSMEMBER - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

REAR SUSPENSION CROSSMEMBER

REMOVAL AND INSTALLATION
Pre-removal Operation Main Muffler, Centre Exhaust Pipe Removal (Refer to GROUP 15, Exhaust pipe and Main Muffler ). Control Link, Upper Arm, Lower Arm Removal (Refer to ). Stabilizer Bar Removal (Refer to ). Fuel Filler Neck Protector Removal (Except for Brazil and Chile, refer to GROUP 13D, Fuel Tank ). (For Brazil and Chile, refer to GROUP 13D, Fuel Tank ). | Post-installation Operation Fuel Filler Neck Protector Installation (Except for Brazil and Chile, refer to GROUP 13D, Fuel Tank ). (For Brazil and Chile, refer to GROUP 13D, Fuel Tank ). Stabilizer Bar Installation (Refer to ). Control Link, Upper Arm, Lower Arm Installation (Refer to ). Main Muffler, Centre Exhaust Pipe Installation (Refer to GROUP 15, Exhaust pipe and Main Muffler ). Rear Wheel Alignment Check and Adjustment (Refer to ).
<2000>
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Dynamic damper <4WD>
|  | 2. | Differential support arm connecting bolt <4WD>
|  | 3. | Rear suspension crossmember
|  | 4. | Differential support arm <4WD>
|  | 5. | Plug
<2400>
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Dynamic damper
|  | 2. | Differential support arm connecting bolt
|  | 3. | Rear suspension crossmember
|  | 4. | Differential support arm
|  | 5. | Plug

[34] REAR SUSPENSION - - REAR SUSPENSION CROSSMEMBER - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation