[35A] SERVICE BRAKE - - BRAKE PEDAL | PRINT PAGE / INDEX / PRIOR / NEXT

BRAKE PEDAL A brake pedal retraction suppression mechanism that minimizes the retraction of the brake pedal in the event of a frontal collision has been adopted to reduce the shock to the feet of the driver. If the brake booster section is pushed in by retraction of the engine, etc. in the event of a collision, the fixing bolt on the support bracket is separated from the reinforcing bracket. The brake pedal bracket hits the support bracket and does not move backwards, and the tread surface of the brake pedal does not move backwards or upwards.

[35A] SERVICE BRAKE - - BRAKE PEDAL | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation