[0] GENERAL - - VEHICLE IDENTIFICATION | PRINT PAGE / INDEX / PRIOR / NEXT

VEHICLE IDENTIFICATION
MODELS
FOR GENERAL EXPORT (Except for Hong Kong, Brunei, Singapore, Malaysia, Brazil, South Africa and Argentina)
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU4W | XRHEZL/R | 4G64-SOHC (2,351 mL) | W4A42 <4WD, INVECS-II 4A/T> | MPI
CU5W | XRMYZL | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T>
XRHYZL
XRHJZL
(For Hong Kong, Brunei, Singapore and Malaysia)
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU2W* | LRMER1D | 4G63-SOHC-Non-Turbo (1,997 mL) | F4A42 <2WD, INVECS-II 4A/T> | MPI
LYXFZR1D | 4G63-DOHC-Turbo (1,997 mL) | W5A51 <4WD, INVECS-II 5A/T>
CU5W* | XRHYZR1D | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T>
(For Brazil)
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU5W | XRMYZL1F | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T> | MPI
XRHYZL1F
(For South Africa)
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU5W | XRMYZR6S | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T> | MPI
XRHYZR6S
(For Argentina)
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU5W | XRHYZL6A | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T> | MPI
FOR GCC
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU5W | XRMYZLW | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T> | MPI
XRHYZLW
FOR NEW ZEALAND
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU2W* | LRMER1D | 4G63-SOHC-Non-Turbo (1,997 mL) | F4A42 <2WD, INVECS-II 4A/T> | MPI
LYXFZR1D | 4G63-DOHC-Turbo (1,997 mL) | W5A51 <4WD, INVECS-II 5A/T>
CU5W | XRMYZR8 | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T>
XRHYZR8
XRXYZR8
FOR AUSTRALIA
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU5W | XRMYZR8 | 4G69-SOHC-MIVEC (2,351 mL) | W4A4B <4WD, INVECS-II 4A/T> | MPI
XRHYZR8
XRXYZR8
NOTE: * indicates the vehicles as "Hong Kong spec." in the running text.

[0] GENERAL - - VEHICLE IDENTIFICATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation