[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

SPECIAL TOOLS
Tool | No. | Name | Application
--- | --- | --- | ---
| MB990784 | Ornament remover | Removal of cover.
| MB990803 | Steering wheel puller | Steering wheel disconnection
| MB991502 | MUT-II sub assembly | Reading and erasing diagnosis code Reading trouble period Reading erase times
| MB991955 A: MB991824 B: MB991827 C: MB991910 D: MB991911 E: MB991825 F: MB991826 | MUT-III sub-assembly A: Vehicle Communication Interface (V. C. I.) B: MUT-III USB cable C: MUT-III main harness A (Vehicles with CAN communication system) D: MUT-III main harness B (Vehicles without CAN communication system) E: MUT-III measurement adapter F: MUT-III trigger harness | Checking diagnosis codes CAUTION If you connect MUT-III main harness A to a vehicle without CAN communication system to use the MUT-III, a pulse signal may interfere with the simulated vehicle speed lines, thus causing the MUT-III inoperative. Therefore, use the MUT-III main harness B (MB991911) instead.
| MB991865 | Dummy resistor | SRS air bag and seat belt with pre-tensioner circuit check
| MB991866 | Resistor harness | SRS air bag circuit check
| MB991884 | Resistor harness (For Pre-tensioner) | Seat belt with pre-tensioner circuit check
| MB991885 | Pre-tensioner adapter harness | Deployment of seat belt with pre-tensioner inside the vehicle Deployment of seat belt with pre-tensioner outside the vehicle
| MB991223 A: MB991219 B: MB991220 C: MB991221 D: MB991222 | Harness set A: Test harness B: LED harness C: LED harness adapter D: Probe | Checking the continuity and measuring the voltage at the SRS-ECU harness connector
| MB686560 | SRS air bag adapter harness | Deployment of air bag module (Front passenger's side) inside the vehicle Deployment of air bag module (Front passenger's side) outside the vehicle

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation