[1] PRE-DELIVERY INSPECTION - - ROAD TEST - 29. BRAKES | PRINT PAGE / INDEX / PRIOR / NEXT

| 29. BRAKES Service Brake Put the vehicle in gear and apply the brakes while the vehicle is in motion. Be sure brake operation is smooth and positive. Parking Brake Stop the vehicle on a steep incline. With the service brakes firmly applied, place the transmission in "N" position, and set the parking brakes. Slowly release the service brakes to see if the parking brakes will hold.

[1] PRE-DELIVERY INSPECTION - - ROAD TEST - 29. BRAKES | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation