[17] ENGINE AND EMISSION CONTROL - - ACCELERATOR SYSTEM - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

ACCELERATOR SYSTEM

GENERAL INFORMATION
<4G63, 4G64, 4G69-L.H. DRIVE VEHICLES> The accelerator system is a cable and suspended pedal combination. Plastic bushing and rubber damper have been attached to the end of the accelerator cable, to prevent noise and vibration when the cable and accelerator arm contact. CONSTRUCTION DIAGRAM
<4G69-R.H. DRIVE VEHICLES> For the accelerator system, an electronic throttle valve control system has been adopted, eliminating of an accelerator cable. This system detects the amount of the accelerator pedal movement by using an accelerator pedal-position sensor (APS) in the accelerator pedal assembly for electronic control of the throttle valve angle. CONSTRUCTION DIAGRAM

[17] ENGINE AND EMISSION CONTROL - - ACCELERATOR SYSTEM - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation