[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - TROUBLESHOOTING - TROUBLE SYMPTOM CHART | PRINT PAGE / INDEX / PRIOR / NEXT

TROUBLE SYMPTOM CHART
Symptom | Inspection Procedure No. | Reference Page
--- | --- | ---
Power of CD or tape player and radio assembly does not turn ON when the ignition switch is in the "ACC" position or "ON" position. | 1 |
No sound from one speaker. <L.H.drive vehicles for Argentina and R.H.drive vehicles> | 2 |
No sound from one speaker. <L.H.drive vehicles (Except for Argentina> | 3 |
Noise | Noise appears at certain places when traveling (AM). | 4 |
Noise is preset while moving (FM). | 5 |
Mixed with noise, only at night (AM). | 6 |
Broadcasts can be heard but both AM and FM have a lot of noise. | 7 |
There is more noise on either AM or FM. | 8 |
There is noise when starting the engine. | 9 |
Some noise appears when there is vibration or shocks during traveling. | 10 |
Noise sometimes appears on FM during traveling. | 11 |
Ever-present noise. | 12 |
Radio | There is noise but no reception for both AM and FM or no sound from AM, or no sound from FM. | 13 |
Poor reception. | 14 |
Distortion on AM or on both AM and FM. | 15 |
Distortion on FM only. | 16 |
Using the auto select function, too few automatic stations are selected. | 17 |
Preset stations are erased. | 18 |
Tape player | Cassette tape can not be inserted. | 19 |
Sound quality is poor, or sound is weak. | 20 |
Cassette tape can not be ejected. | 21 |
Uneven revolution. Tape speed is fast or slow. | 22 |
Automatic search does not work. | 23 |
Malfunction of the auto reverse. | 24 |
Tape gets caught in mechanism. | 25 |
CD player | CD can not be inserted. | 26 |
No sound (CD only). | 27 |
CD sound skips. | 28 |
Sound quality is poor. | 29 |
CD cannot be ejected. | 30 |

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - TROUBLESHOOTING - TROUBLE SYMPTOM CHART | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation