[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - HYDRAULIC UNIT - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

HYDRAULIC UNIT

REMOVAL AND INSTALLATION
<L.H. DRIVE VEHICLES> NOTE: The ABS-ECU is integrated in the hydraulic unit.
Pre-removal Operation Brake Fluid Draining | Post-installation Operation Brake Fluid Filling Bake Line Bleeding (Refer to GROUP 35A, On-vehicle Service - Bleeding .) Hydraulic Unit Check (Refer to .)
|  |  | Removal steps
--- | --- | --- | ---
<<A>> |  | 1. | Harness connector
| >>A<< | 2. | Brake pipe connection
<<B>> |  | 3. | Hydraulic unit and ABS-ECU
|  | 4. | Hydraulic unit bracket assembly
<R.H. DRIVE VEHICLES> NOTE: The ABS-ECU is integrated in the hydraulic unit.
Pre-removal Operation Brake Fluid Draining Air Cleaner Removal (Refer to GROUP 15, Air Cleaner <2000-SOHC or 2400-Except MIVEC>, <2000-DOHC> or <2400-MIVEC>.) | Post-installation Operation Brake Fluid Filling Brake Line Bleeding (Refer to GROUP 35A, On-vehicle Service - Bleeding .) Air Cleaner Installation (Refer to GROUP 15, Air Cleaner <2000-SOHC or 2400-Except MIVEC>, <2000-DOHC> or <2400-MIVEC>.) Hydraulic Unit Check (Refer to .)
|  |  | Removal steps
--- | --- | --- | ---
<<A>> |  | 1. | Harness connector
| >>A<< | 2. | Brake pipe connection
<<B>> |  | 3. | Hydraulic unit and ABS-ECU
|  | 4. | Hydraulic unit bracket assembly
| REMOVAL SERVICE POINTS
| <<A>> HARNESS CONNECTOR DISCONNECTION
| Move the lock lever of the ABS-ECU connector as shown in the illustration, and then disconnect the harness connector.
| <<B>> HYDRAULIC UNIT AND ABS-ECU REMOVAL WARNING The hydraulic unit is heavy. Use care when removing it. CAUTION The hydraulic unit cannot be disassembled. Never loosen its nuts or bolts. Do not drop or shock the hydraulic unit. Do not turn the hydraulic unit upside down or lay it on its side.
| INSTALLATION SERVICE POINT
| >>A<< BRAKE PIPE CONNECTION
| Connect the pipes to the hydraulic unit assembly as shown in the illustration. From the master cylinder (secondary) To the front brake (LH) To the rear brake (RH) To the rear brake (LH) To the front brake (RH) From the master cylinder (primary)

[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - HYDRAULIC UNIT - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation