[11D] ENGINE OVERHAUL <4G6-DOHC> - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

SPECIAL TOOLS
Tool | Number | Name | Use
--- | --- | --- | ---
| MD998781 | Flywheel stopper | Retention of flywheel
| MD998778 | Crankshaft sprocket puller | Removal of crankshaft sprocket and crankshaft sprocket B
| MD998785 | Sprocket stopper | Retention of counterbalancer shaft sprocket
| MD998767 | Tension pulley socket wrench | Manipulation of tensioner pulley during adjustment of timing belt tension
| MD998738 | Set screw | Retention of tensioner arm and auto-tensioner during timing belt installation
| MD998713 | Camshaft oil seal installer | Installation of camshaft oil seal
| MD998442 | Air bleed wire | Air bleeding of lash adjuster
| MB991654 | Cylinder head bolt wrench | Removal and installation of cylinder head bolts
| MD998772 | Valve spring compressor | Compression of valve spring
| MD998735 | Valve spring compressor | Compression of valve spring
| MD998737 | Valve stem seal installer | Installation of valve stem seal
| MD998162 | Plug wrench | Removal and installation of front case plug cap (Use with MD998783.)
| MD998783 | Plug wrench retainer | Removal and installation of front case plug cap (Use with MD998162.)
| MD998371 | Silent shaft bearing puller | Removal of counterbalancer shaft front bearing
| MD998372 | Silent shaft bearing puller | Removal of counterbalancer shaft front and rear bearings
| MB991603 | Silent shaft bearing installer stopper | Guide and stopper for removal and press-fitting of counterbalancer shaft rear bearing
| MD998705 | Silent shaft bearing installer | Press-fitting of counterbalancer shaft front and rear bearings
| MD998375 | Crankshaft front oil seal installer | Installation of crankshaft front oil seal
| MD998285 | Crankshaft front oil seal guide | Guide for installation of crankshaft front oil seal
| MD998780 | Piston pin setting tool | Removal and press-fitting of piston pin
| MD998776 | Crankshaft rear oil seal installer | Installation of crankshaft rear oil seal
| MB990938 | Handle | Installation of crankshaft rear oil seal (Use with MD998776.)

[11D] ENGINE OVERHAUL <4G6-DOHC> - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation