[52A] INTERIOR - - REAR SEAT ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

REAR SEAT ASSEMBLY

REMOVAL AND INSTALLATION
<VEHICLES FOR SOUTH AFRICA, ARGENTINA AND AUSTRALIA>
|  | 1. | Head restraint
|  |  | Removal steps
--- | --- | --- | ---
| >>A<< | 2. | Rear seat cushion assembly
|  | 3. | Inner seat belt and centre seat belt installation bolt
|  | 4. | Rear seatback assembly (L.H.)
|  | 5. | Rear seatback assembly (R.H.)
|  | 6. | Rear seat hook
<EXCEPT VEHICLES FOR SOUTH AFRICA, ARGENTINA AND AUSTRALIA>
|  | 1. | Head restraint
|  |  | Removal steps
--- | --- | --- | ---
| >>A<< | 2. | Rear seat cushion assembly
|  | 3. | Rear seatback assembly (L.H.)
|  | 4. | Rear seatback assembly (R.H.)
|  | 5. | Rear seat hook
| INSTALLATION SERVICE POINT
| >>A<< REAR SEAT CUSHION ASSEMBLY INSTALLATION
| Fit the rear seat cushion into the rear seat hook securely.

[52A] INTERIOR - - REAR SEAT ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation