[0] GENERAL - - PRECAUTIONS BEFORE SERVICE - APPLICATION OF ANTI-CORROSION AGENTS AND UNDERCOATS | PRINT PAGE / INDEX / PRIOR / NEXT

| APPLICATION OF ANTI-CORROSION AGENTS AND UNDERCOATS If oil or grease gets onto the oxygen sensor, it will cause a drop in the performance of the sensor. Cover the oxygen sensor with a protective cover when applying anti-corrosion agents and undercoats.

[0] GENERAL - - PRECAUTIONS BEFORE SERVICE - APPLICATION OF ANTI-CORROSION AGENTS AND UNDERCOATS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation