[23C] AUTOMATIC TRANSMISSION OVERHAUL <W5A5> - - SECOND BRAKE - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

SECOND BRAKE

DISASSEMBLY AND REASSEMBLY
|  |  | Disassembly steps
--- | --- | --- | ---
|  | 1. | Second brake retainer
| >>A<< | 2. | D-ring
|  | 3. | Second brake piston
| >>A<< | 4. | D-ring
| REASSEMBLY SERVICE POINT
| >>A<< D-RING INSTALLATION Apply ATF, blue petrolatum jelly or white Vaseline to the D-rings, and handle them carefully to avoid damage during installation.

[23C] AUTOMATIC TRANSMISSION OVERHAUL <W5A5> - - SECOND BRAKE - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation