[23B] AUTOMATIC TRANSMISSION OVERHAUL <F4A4/W4A4> - - VALVE BODY - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

VALVE BODY

DISASSEMBLY AND REASSEMBLY
|  |  | Disassembly steps
--- | --- | --- | ---
|  | 1. | Solenoid valve support
<<A>> | >>C<< | 2. | Underdrive solenoid valve
<<A>> | >>C<< | 3. | Second solenoid valve
<<A>> | >>C<< | 4. | Damper clutch control solenoid valve
<<A>> | >>C<< | 5. | Overdrive solenoid valve
<<A>> | >>C<< | 6. | Low-reverse solenoid valve
|  | 7. | Manual valve
|  | 8. | Cover
|  | 9. | Plate
|  | 10. | Outside valve body assembly
| >>B<< | 11. | Steel ball (orifice check ball)
| >>B<< | 12. | Spring
|  | 13. | Plate
| >>A<< | 14. | Damping valve
| >>A<< | 15. | Damping valve spring
| >>A<< | 16. | Steel ball (line relief)
| >>A<< | 17. | Spring
| >>A<< | 18. | Steel ball (orifice check ball)
| >>A<< | 19. | Spring
|  | 20. | Inside valve body assembly
|  |  | Disassembly steps
--- | --- | --- | ---
|  | 21. | Roller
|  | 22. | Damper clutch control valve sleeve
|  | 23. | Damper clutch control valve
|  | 24. | Damper clutch control valve spring
|  | 25. | Plate
|  | 26. | Screw
|  | 27. | Regulator valve spring
|  | 28. | Regulator valve
|  | 29. | Plate
|  | 30. | Fail-safe valve A sleeve
|  | 31. | Fail-safe valve A2
|  | 32. | Fail-safe valve A spring
|  | 33. | Fail-safe valve A1
|  | 34. | Plate
|  | 35. | Plug
|  | 36. | Torque converter valve
|  | 37. | Torque converter valve spring
|  | 38. | Plate
|  | 39. | Fail-safe valve B sleeve
|  | 40. | Fail-safe valve B
|  | 41. | Inside valve body
|  | 42. | Roller
|  | 43. | Overdrive pressure control valve sleeve
|  | 44. | Overdrive pressure control valve
|  | 45. | Overdrive pressure control valve spring
|  | 46. | Roller
|  | 47. | Low-reverse pressure control valve sleeve
|  | 48. | Low-reverse pressure control valve
|  | 49. | Low-reverse pressure control valve spring
|  | 50. | Plate
|  | 51. | Plug
|  | 52. | Switch valve
|  | 53. | Roller
|  | 54. | Underdrive pressure control valve sleeve
|  | 55. | Underdrive pressure control valve
|  | 56. | Underdrive pressure control valve spring
|  | 57. | Roller
|  | 58. | Second pressure control valve sleeve
|  | 59. | Second pressure control valve
|  | 60. | Second pressure control valve spring
|  | 61. | Outside valve body
| DISASSEMBLY SERVICE POINT
| <<A>> SOLENOID VALVE REMOVAL
| Mark each solenoid valve with white paint to identify its location.
| REASSEMBLY SERVICE POINTS
| >>A<< SPRING/STEEL BALL/DAMPING VALVE/DAMPING VALVE SPRING INSTALLATION
| Install the springs (two pieces), steel balls (two pieces), damping valve, and damping valve spring into the locations indicated in the illustration.
| >>B<< SPRING/STEEL BALLS INSTALLATION
| Install the springs (two pieces) and steel balls (three pieces) into the locations indicated in the illustration.
| >>C<< SOLENOID VALVES INSTALLATION
| Install the solenoid valves according to the markings that have been made during disassembly.
No. | Solenoid valve
--- | ---
1 | Underdrive solenoid valve
2 | Second solenoid valve
3 | Damper clutch control solenoid valve
4 | Overdrive solenoid valve
5 | Low-reverse solenoid valve

[23B] AUTOMATIC TRANSMISSION OVERHAUL <F4A4/W4A4> - - VALVE BODY - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation