[51] EXTERIOR - - REAR BUMPER ASSEMBLY - REAR BUMPER ASSEMBLY - REMOVAL AND INSTALLATION <2000> | PRINT PAGE / INDEX / PRIOR / NEXT

REAR BUMPER ASSEMBLY

REMOVAL AND INSTALLATION <2000>
|  |  | Removal steps
--- | --- | --- | ---
|  | • | Rear combination lamp (Refer to GROUP 54A, Rear combination lamp ).
|  | • | Rear end trim (Refer to 52A, Trims ).
|  | 1. | Rear splash shield
|  | • | Licence lamp connector connection
|  | 2. | Rear bumper assembly
|  | • | Ventilation cap (Refer to GROUP 52A, Trims ).
<<A>> |  | 3. | Clips
| REMOVAL SERVICE POINT
| <<A>> CLIPS REMOVAL
| Remove the clip with a pair of pliers by removing the thumb of the clip from the cabin side.

[51] EXTERIOR - - REAR BUMPER ASSEMBLY - REAR BUMPER ASSEMBLY - REMOVAL AND INSTALLATION <2000> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation