[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS> - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 2: When the ignition key is at a position other than the LOCK (OFF) position, the selector lever cannot be moved from the P to the R position even though the brake pedal is being depressed. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 2: When the ignition key is at a position other than the LOCK (OFF) position, the selector lever cannot be moved from the P to the R position even though the brake pedal is being depressed.
COMMENTS ON TROUBLE SYMPTOM The cause is probably a malfunction of the selector lever assembly, transmission control cable, shift lock cable, key interlock cable or ignition key cylinder lock bar.
Possible causes Malfunction of selector lever assembly Malfunction of transmission control cable Malfunction of shift lock cable Malfunction of key interlock cable Malfunction of lock bar
DIAGNOSIS Check by referring to the possible causes.

[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS> - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 2: When the ignition key is at a position other than the LOCK (OFF) position, the selector lever cannot be moved from the P to the R position even though the brake pedal is being depressed. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation