[23C] AUTOMATIC TRANSMISSION OVERHAUL <W5A5> - - SNAP RING, SPACER, THRUST WASHER, THRUST RACE AND PRESSURE PLATE FOR ADJUSTING | PRINT PAGE / INDEX / PRIOR / NEXT

SNAP RING, SPACER, THRUST WASHER, THRUST RACE AND PRESSURE PLATE FOR ADJUSTING
SNAP RING (FOR ADJUSTMENT OF BRAKE REACTION PLATE END PLAY)
Thickness mm | Identification symbol |  | Thickness mm | Identification symbol
--- | --- | --- | --- | ---
2.2 | None |  | 2.4 | Brown
2.3 | Blue | 2.5 | None
PRESSURE PLATE (FOR ADJUSTING OF LOW-REVERSE BRAKE END PLAY)
Thickness mm | Identification symbol |  | Thickness mm | Identification symbol
--- | --- | --- | --- | ---
1.6 | F |  | 2.4 | B
1.8 | E | 2.6 | A
2.0 | D | 2.8 | 0
2.2 | C | 3.0 | 1
PRESSURE PLATE (FOR ADJUSTING OF SECOND BRAKE END PLAY)
Thickness mm | Identification symbol |  | Thickness mm | Identification symbol
--- | --- | --- | --- | ---
2.4 | P |  | 3.0 | T
2.6 | R | 3.2 | U
2.8 | S | 3.4 | V
THRUST RACE (FOR ADJUSTING OF UNDERDRIVE SUN GEAR END PLAY)
Thickness mm | Identification symbol |  | Thickness mm | Identification symbol
--- | --- | --- | --- | ---
1.6 | - |  | 2.2 | -
1.7 | - | 2.3 | -
1.8 | - | 2.4 | -
1.9 | - | 2.5 | -
2.0 | - | 2.6 | -
2.1 | - |
THRUST WASHER (FOR ADJUSTING OF INPUT SHAFT END PLAY)
Thickness mm | Identification symbol |  | Thickness mm | Identification symbol
--- | --- | --- | --- | ---
1.8 | 18 |  | 2.4 | 24
2.0 | 20 | 2.6 | 26
2.2 | 22 | 2.8 | 28
SPACERS (FOR ADJUSTING OF DIFFERENTIAL CASE PRELOAD)
Thickness mm | Identification symbol |  | Thickness mm | Identification symbol
--- | --- | --- | --- | ---
0.83 | 83 |  | 1.10 | 10
0.86 | 86 | 1.13 | 13
0.89 | 89 | 1.16 | 16
0.92 | 92 | 1.19 | 19
0.95 | 95 | 1.22 | 22
0.98 | 98 | 1.25 | 25
1.01 | 01 | 1.28 | 28
1.04 | 04 | 1.31 | 31
1.07 | 07 |
SNAP RING (FOR ADJUSTING OF UNDERDRIVE CLUTCH END PLAY AND OVERDRIVE CLUTCH END PLAY )
Thickness mm | Identification symbol |  | Thickness mm | Identification symbol
--- | --- | --- | --- | ---
1.6 | Brown |  | 2.4 | Blue
1.7 | None | 2.5 | Brown
1.8 | Blue | 2.6 | None
1.9 | Brown | 2.7 | Blue
2.0 | None | 2.8 | Brown
2.1 | Blue | 2.9 | None
2.2 | Brown | 3.0 | Blue
2.3 | None |
SNAP RING (FOR ADJUSTING OF REVERSE AND OVERDRIVE CLUTCH RETURN SPRING RETAINER END PLAY)
Thickness mm | Identification symbol |  | Thickness mm | Identification symbol
--- | --- | --- | --- | ---
1.43 | Brown |  | 1.53 | Blue
1.48 | None | 1.58 | Brown
SNAP RING (FOR ADJUSTING OF REVERSE CLUTCH END PLAY)
Thickness mm | Identification symbol |  | Thickness mm | Identification symbol
--- | --- | --- | --- | ---
1.6 | None |  | 2.3 | Blue
1.7 | Blue | 2.4 | Brown
1.8 | Brown | 2.5 | None
1.9 | None | 2.6 | Blue
2.0 | Blue | 2.7 | Brown
2.1 | Brown | 2.8 | None
2.2 | None |
SNAP RING (FOR ADJUSTING OF DIRECT CLUTCH END PLAY)
Thickness mm | Identification symbol |  | Thickness mm | Identification symbol
--- | --- | --- | --- | ---
1.9 | Brown |  | 2.5 | Brown
2.0 | None | 2.6 | None
2.1 | Blue | 2.7 | Blue
2.2 | Brown | 2.8 | Brown
2.3 | None | 2.9 | None
2.4 | Blue | 3.0 | Blue
SPACER (FOR ADJUSTING BACKLASH BETWEEN CENTRE DIFFERENTIAL GEARS AND PINION)
Thickness mm | Identification symbol |  | Thickness mm | Identification symbol
--- | --- | --- | --- | ---
0.56 - 0.64 | - |  | 0.86 - 0.94 | -
0.66 - 0.74 | - | 0.96 - 1.04 | -
0.76 - 0.84 | - | 1.06 - 1.14 | -

[23C] AUTOMATIC TRANSMISSION OVERHAUL <W5A5> - - SNAP RING, SPACER, THRUST WASHER, THRUST RACE AND PRESSURE PLATE FOR ADJUSTING | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation