[2] BODY DIMENSIONS - - TYPE B (ACTUAL-MEASUREMENT DIMENSIONS) - SIDE BODY <2000> | PRINT PAGE / INDEX / PRIOR / NEXT

SIDE BODY <2000>
No. | Standard measurement point | Hole shape | Size mm
--- | --- | --- | ---
36 | Front pillar positioning notch (upper) | - | -
37 | Front pillar positioning notch (lower) | - | -
38 | Side roof rail positioning notch (front) | - | -
39 | Side sill positioning notch (front) | - | -
40 | Centre pillar positioning notch (upper) | - | -
41 | Centre pillar positioning notch (lower) | - | -
42 | Side roof rail positioning notch (rear) | - | -
43 | Side sill positioning notch (rear) | - | -
44 | Quarter panel positioning notch (upper) | - | -
45 | Quarter panel positioning notch (lower) | - | -
46 | Centre of front door hinge mounting hole (upper) | Round | 11
47 | Centre of front door hinge mounting hole (lower) | Round | 11
48 | Centre of front door hinge mounting hole (lower) | Round | 11
49 | Centre of rear door hinge mounting hole (lower) | Round | 11
50 | Centre of rear door switch mounting hole | Round | 5

[2] BODY DIMENSIONS - - TYPE B (ACTUAL-MEASUREMENT DIMENSIONS) - SIDE BODY <2000> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation