[27B] REAR AXLE <4WD> - - SPECIFICATION(S) - LUBRICANTS | PRINT PAGE / INDEX / PRIOR / NEXT

LUBRICANTS
Item | Specified lubricant | Quantity
--- | --- | ---
Rear differential gear oil | Hypoid gear oil API classification GL-5 or higher Above 10°C: SAE 90 Below 10°C: SAE 80W | 0.55 L
Drive shaft BJ joint | Repair kit grease | 75 ± 10 g
Drive shaft TJ joint | Repair kit grease | 110 ± 10 g

[27B] REAR AXLE <4WD> - - SPECIFICATION(S) - LUBRICANTS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation