[0] GENERAL - - PRECAUTIONS BEFORE SERVICE - VEHICLE WASHING | PRINT PAGE / INDEX / PRIOR / NEXT

| VEHICLE WASHING
| If high-pressure car-washing equipment or steam car-washing equipment is used to wash the vehicle, be sure to note the following information in order to avoid damage to plastic components, etc. Spray nozzle distance: Approx. 40 cm or more Spray pressure: 3,900 kPa or less Spray temperature: 82°C or less Time of concentrated spray to one point: within 30 sec.

[0] GENERAL - - PRECAUTIONS BEFORE SERVICE - VEHICLE WASHING | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation