[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 19: Cassette Tape can Not be Inserted. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 19: Cassette Tape can Not be Inserted.
DIAGNOSIS PROCEDURE
STEP 1. Check that there are any foreign objects inside the tape player. NOTE: Attempting to eliminate a foreign object (e.g., a coin or clip, etc.) in the tape player may damage the mechanism. The player should be taken to a service dealer for repair. Q: Are there any foreign objects inside the tape player? YES: There are any foreign objects inside the tape player, remove the object(s). A cassette tape should be inserted normally. NO: Go to Step 2.
STEP 2. Check that the radio and tape player works when another tape is inserted. NOTE: Check that the tape label is not loose, that the tape case is not deformed and that the tape is tightly wound. Also, tape with a length of C-120 or greater can often get caught in the mechanism and should not be used. Q: Does the tape player work if another tape is inserted? YES: The cassette tape used is defective. A cassette tape should be inserted normally. NO: Replace the radio with tape player. A cassette tape should be inserted normally.

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 19: Cassette Tape can Not be Inserted. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation