[55B] AUTOMATIC AIR CONDITIONER - - TROUBLESHOOTING - DIAGNOSIS CODE CHART | PRINT PAGE / INDEX / PRIOR / NEXT

DIAGNOSIS CODE CHART
Code No. | Diagnostic item | Reference page
--- | --- | ---
11 | Interior temperature senor system (open circuit) |
12 | Interior temperature sensor system (short circuit) |
13 | Outside thermo sensor system (open circuit) |
14 | Outside thermo sensor system (short circuit) |
15 | Heater water temperature sensor system (open circuit) |
16 | Heater water temperature sensor system (short circuit) |
21 | Air thermo sensor system (open circuit) |
22 | Air thermo sensor system (short circuit) |
31 | Air mixing door control motor and potentiometer sensor system |
32 | Mode selection damper control motor and potentiometer sensor system |
41 | Air mixing door control motor and potentiometer activating system |
42 | Mode selection damper control motor and potentiometer activating system |

[55B] AUTOMATIC AIR CONDITIONER - - TROUBLESHOOTING - DIAGNOSIS CODE CHART | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation