[37] POWER STEERING - - LUBRICANTS | PRINT PAGE / INDEX / PRIOR / NEXT

LUBRICANTS
Item | Specified lubricant | Quantity
--- | --- | ---
Power steering fluid | ATF DEXRON III or DEXRON II | 1.0 L
Steering gear | Bearing | ATF DEXRON III or DEXRON II | As required
O-ring and seal ring
Oil seal
Special tool (MB991213)
Pinion and valve assembly seal ring part
Bellows | Silicon grease | As required
Tie rod end ball joint | Multipurpose grease SAE J310, NLGI No.2 or equivalent | As required
Oil pump | Friction surface of rotor vane, cam ring and pump cover | ATF DEXRON III or DEXRON II | As required
O-ring

[37] POWER STEERING - - LUBRICANTS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation