[15] INTAKE AND EXHAUST - - INTERCOOLER - REMOVAL AND INSTALLATION <4G63-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

INTERCOOLER

REMOVAL AND INSTALLATION <4G63-DOHC>
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Intercooler, intercooler cover, intercooler bracket, intercooler outlet air hose A and intercooler intake air hose assembly
|  | 2. | Intercooler outlet air hose A
|  | 3. | Intercooler intake air hose
|  | 4. | Intercooler cover
|  | 5. | Intercooler bracket
|  | 6. | Intercooler
|  | • | Air duct (Refer to )
|  | • | Battery and battery tray
|  | 7. | Intercooler outlet air hose B
|  | 8. | Vacuum hose connection
|  | 9. | Air by-pass valve assembly
|  | 10. | Rear bracket
|  | 11. | Front bracket

[15] INTAKE AND EXHAUST - - INTERCOOLER - REMOVAL AND INSTALLATION <4G63-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation