[36] PARKING BRAKES - - PARKING BRAKE CABLE - REMOVAL AND INSTALLATION <L.H. drive vehicles> | PRINT PAGE / INDEX / PRIOR / NEXT

PARKING BRAKE CABLE

REMOVAL AND INSTALLATION <L.H. drive vehicles>
<Vehicles with rear drum brakes>
Pre-removal Operation Rear Floor Console Assembly Removal (Refer to GROUP 52A, Floor Console Assembly ). | Post-installation Operation Parking Brake Lever Stroke adjustment (Refer to ). Rear Floor Console Assembly Installation (Refer to GROUP 52A, Floor Console Assembly ).
|  |  | Removal steps
--- | --- | --- | ---
|  | • | Loosen the adjusting nuts.
|  | 1. | Brake drum
<<A>> |  | 2. | Parking brake cable connection
|  | 3. | Parking brake cable connection
|  | 4. | Parking brake cable
<Vehicles with rear drum-in disc brakes>
Pre-removal Operation Rear Floor Console Assembly Removal (Refer to GROUP 52A, Floor Console Assembly ). | Post-installation Operation Parking Brake Lever Stroke adjustment (Refer to ). Rear Floor Console Assembly Installation (Refer to GROUP 52A, Floor Console Assembly ).
|  |  | Removal steps
--- | --- | --- | ---
|  | • | Shoe and lining assembly (Refer to ).
|  | • | Loosen the adjusting nuts.
|  | • | Turn up the driver's side carpet.
|  | 1. | Parking brake cable connection
|  | 2. | Clip
|  | 3. | Protector B
|  | 4. | Parking brake cable connection
|  | 5. | Protector C
|  | 6. | Rear parking brake cable assembly
| REMOVAL SERVICE POINT
| <<A>> PARKING BRAKE CABLE CONNECTION REMOVAL <Vehicles with rear drum brakes>
| Withdraw the parking brake cable from the backing plate. NOTE: Insert a 10 mm-wrench into the parking brake cable to facilitate the cable withdrawal.

[36] PARKING BRAKES - - PARKING BRAKE CABLE - REMOVAL AND INSTALLATION <L.H. drive vehicles> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation