[11D] ENGINE OVERHAUL <4G6-DOHC> - - ALTERNATOR AND IGNITION SYSTEM - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

ALTERNATOR AND IGNITION SYSTEM

REMOVAL AND INSTALLATION
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Oil level gauge
|  | 2. | O-ring
|  | 3. | Oil level gauge guide
|  | 4. | O-ring
|  | 5. | Idler pulley
|  | 6. | Cap
|  | 7. | Auto-tensioner assembly
|  | 8. | Water pump pulley
|  | 9. | Alternator brace
|  | 10. | Alternator
|  | 11. | Crankshaft pulley
|  | 12. | Center cover
|  | 13. | Spark plug cable
|  | 14. | Ignition coil
|  | 15. | Spark plug

[11D] ENGINE OVERHAUL <4G6-DOHC> - - ALTERNATOR AND IGNITION SYSTEM - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation