[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 30: CD cannot be Ejected. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 30: CD cannot be Ejected.
DIAGNOSIS PROCEDURE
Check the power of ignition switch "ACC". Q: Does the radio and CD player power turn ON when the ignition switch is in the "ACC" or "ON" position? YES: Replace the radio with CD player. Check that a CD can be ejected normally. NO: Check the power supply circuit. Refer to Inspection Procedure 1 .

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 30: CD cannot be Ejected. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation