[23B] AUTOMATIC TRANSMISSION OVERHAUL <F4A4/W4A4> - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Item | Standard value
--- | ---
Brake reaction plate end play mm | 0 - 0.16
Second brake end play mm | 0.79 - 1.25
Low-reverse brake end play mm | 1.65 - 2.11
Output shaft preload mm | 0.01 - 0.09
Underdrive sun gear end play mm | 0.25 - 0.45
Input shaft end play mm | 0.70 - 1.45
Differential case preload mm | 0.045 - 0.105
Underdrive clutch piston end play mm | 1.6 - 1.8
Overdrive clutch return spring retainer end play mm | 0 - 0.09
Overdrive clutch end play mm | 1.6 - 1.8
Reverse clutch end play mm | 1.5 - 1.7
Backlash between differential side gear and pinion mm | 0.025 - 0.150

[23B] AUTOMATIC TRANSMISSION OVERHAUL <F4A4/W4A4> - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation