[34] REAR SUSPENSION - - ON-VEHICLE SERVICE - STABILIZER LINK BALL JOINT DUST COVER INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| STABILIZER LINK BALL JOINT DUST COVER INSPECTION Check dust covers for cracks or damage by pushing it with your finger. If a dust cover is cracked or damaged, replace the stabilizer link. NOTE: Cracks or damage to the dust cover may cause damage to the ball joint.

[34] REAR SUSPENSION - - ON-VEHICLE SERVICE - STABILIZER LINK BALL JOINT DUST COVER INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation