[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - SRS WARNING LAMP CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| SRS WARNING LAMP CHECK
| Check that the SRS warning lamp comes on when the ignition switch is turned ON. Check that the SRS warning lamp illuminates for about 7 seconds and then goes out. If this is not the cause, check the diagnosis codes.

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - SRS WARNING LAMP CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation