[42] BODY - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL INFORMATION
FEATURES
WEIGHT REDUCTION AND HIGH RIGIDITY Use of high-tensile steel panels and steel plate with varying thickness.
REDUCTION OF VIBRATION, NOISE, AND AERODYNAMIC NOISE Effective positioning of sound-deadening materials.
IMPROVEMENTS IN SAFETY Features an impact safety body for the main body. Features a side door beam to boost safety upon side impact. Features an inside lock cable on the front door to prevent door locking due to door deformation upon frontal impact. The impact detection door unlock mechanism is adopted. The one touch power window with safety mechanism (with after key removing function) is used <Vehicles for Hong Kong spec>. The one touch power window with safety mechanism is used <Vehicles for Argentina>. The new power window switch is adopted. The switch enables to open the power window even if the vehicle is submerged <Vehicles for Hong Kong spec and Argentina>.
IMPROVEMENTS IN OPERATION QUALITY Comes with a central door lock with a lock/unlock option in all doors and the tailgate.
IMPROVEMENTS OF PRODUCT PACKAGE AND APPEARANCE The one touch power window is used <Except vehicles for Hong Kong spec and Argentina>. UV-cut glasses are used for the front door window glasses <Vehicles for Hong Kong spec>. Comes with a privacy glass for the rear door window glass, quarter window glass and tailgate glass <Except vehicles for GCC> (some models). Standard sunroof <Except vehicles for Hong Kong spec> (some models). The sunroof and roof window glass are used <Vehicles for Hong Kong spec> (some models). Standard keyless entry system <Except vehicles for Hong Kong spec> (some models). The multi-mode keyless entry system (with door mirror unfolding/folding function and sunroof and power window control function) is used <Vehicles for Hong Kong spec> (some models). The security alarm function is used for the keyless entry system <Vehicles for Hong Kong spec>.

[42] BODY - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation