[2] BODY DIMENSIONS - - TYPE B (ACTUAL-MEASUREMENT DIMENSIONS) - SUSPENSION INSTALLATION DIMENSIONS <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

SUSPENSION INSTALLATION DIMENSIONS <2400>
No. | Standard measurement point | Hole shape | Size mm
--- | --- | --- | ---
3 | Centre of crossmember mounting hole | Round | 18
14 | Tip of crossmember mounting bolt (left) | - | -
15 | Tip of crossmember mounting bolt (right) | - | -
16 | Centre of crossmember mounting hole | Round | 11
17 | Centre of trailing arm mounting hole | Round | 16
18 | Centre of trailing arm mounting hole | Round | 16
19 | Centre of crossmember mounting hole | Round | 28
20 | Centre of crossmember mounting hole | Round | 14
21 | Centre of crossmember mounting hole | Round | 13.5
22 | Centre of crossmember mounting hole | Round | 13.5

[2] BODY DIMENSIONS - - TYPE B (ACTUAL-MEASUREMENT DIMENSIONS) - SUSPENSION INSTALLATION DIMENSIONS <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation