[54A] CHASSIS ELECTRICAL - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL INFORMATION The adoption of new accessories and functions has enhanced a lineup of equipment.
FEATURES
ENHANCED RELIABILITY Adoption of waterproof connector in the engine compartment Installation of fuse box and relay box
ENHANCED VISIBILITY AND SAFETY ENHANCED EASE-OF-USE AND CONVENIENCE Equipped with two headlamps A high mount stop lamp is assembled on the tailgate spoiler The combination meters feature a round speedometer and tachometer with large needle movement angle.
IMPROVEMENTS IN SERVICE QUALITY Installation of diagnostic connectors (two) for MUT-II/III inspection Addition of ignition timing inspection function to the MUT-II/III Adoption of Simplified Wiring System (SWS) to reduce weight and complexity of harnesses
IMPROVEMENTS IN COMMERCIAL VALUE Installation of an engine immobilizer system <Vehicles for South Africa, GCC, Australia and New zealand (2400)> Addition of map lamp and front room lamp Adoption of an electronically tuned AM/FM radio with tape player <Vehicles for GCC: standard, Vehicles for General Export (except for Hong Kong spec. and South Africa): option> or electronically turned AM/FM radio with CD player <Vehicles for Australia and New zealand (2400)> Adoption of CD autochanger <Standard: Vehicles for Australia and New zealand (XLS, LTD model), Option: Vehicles for General Export (except for Hong Kong spec. and South Africa), GCC (GLS model), Australia and New zealand (LS model)> Addition of accessory socket <Vehicles for South Africa>

[54A] CHASSIS ELECTRICAL - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation