[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - DIAGNOSTIC TROUBLE CODE PROCEDURES - Code No.39 Airbags Deployed Simultaneously | PRINT PAGE / INDEX / PRIOR / NEXT

Code No.39 Airbags Deployed Simultaneously
| DIAGNOSIS CODE SET CONDITIONS This code is set when the airbags have deployed simultaneously. If this code is set before the airbags have deployed, an internal failure may have occurred in the SRS-ECU.
| PROBABLE CAUSE Malfunction of the SRS-ECU
| DIAGNOSIS Replace the SRS-ECU (Refer to ).

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - DIAGNOSTIC TROUBLE CODE PROCEDURES - Code No.39 Airbags Deployed Simultaneously | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation