[42] BODY - - FUEL FILLER LID - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

FUEL FILLER LID

REMOVAL AND INSTALLATION
Pre-removal and Post-installation Operation Rear Seat Removal and Installation (Refer to GROUP 52A, Rear Seat .) Front Seat Assembly (Driver's Seat Side) Removal and Installation (Refer to GROUP 52A, Front Seat .) Front Seat Belt Anchor Bolt (Driver's Side) Removal and Installation (Refer to GROUP 52A, Front Seat Belt .) Front Scuff Plate (Driver's Side), Rear Scuff Plate (Driver's Side), Center Pillar Lower Trim (Driver's Side) Removal and Installation (Refer to GROUP 52A, Trims .) Floor Console Removal and Installation (Refer to GROUP 52A, Floor Console .)
|  | Removal steps
--- | --- | ---
|  | 1. | Fuel filler lid panel assembly
|  | 2. | Clip
|  | 3. | Fuel filler lid hook assembly
|  | 4. | Fuel filler lid lock release handle
|  | • | Quarter lower trim (Refer to GROUP 52A, Trims .)
|  | • | Protector C (Refer to GROUP 36, Parking Brake Cable <LH drive vehicles>, <RH drive vehicles>).
|  | 5. | Fuel filler lid lock release cable

[42] BODY - - FUEL FILLER LID - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation