[55B] AUTOMATIC AIR CONDITIONER - - TROUBLESHOOTING - TROUBLE SYMPTOM CHART | PRINT PAGE / INDEX / PRIOR / NEXT

TROUBLE SYMPTOM CHART
Symptom | Inspection procedure number | Reference page
--- | --- | ---
Communication with the MUT-II/III is not possible. | 1 |
The air conditioner does not work at all. | 2 |
A/C outlet air temperature cannot be set. | 3 |
The blower does not work. | 4 |
The blower air volume cannot be changed. | 5 |
When sunlight intensity changes, air outlet temperature does not change. | 6 |
The A/C indicator flashes. | 7 |
The inside/outside air changeover is impossible. | 8 |
Defogger function does not operate. | 9 |
Malfunction of the A/C-ECU power supply system. | 10 |

[55B] AUTOMATIC AIR CONDITIONER - - TROUBLESHOOTING - TROUBLE SYMPTOM CHART | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation