[11F] ENGINE OVERHAUL <4G69> - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL INFORMATION
VEHICLE AND ENGINE MODELS
Vehicle name | Vehicle model | Engine model | Displacement mL | Specification
--- | --- | --- | --- | ---
Outlander | CU5W | 4G69-2 | 2,378 | Single overhead camshaft, 16-valve

[11F] ENGINE OVERHAUL <4G69> - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation