[54A] CHASSIS ELECTRICAL - - BATTERY | PRINT PAGE / INDEX / PRIOR / NEXT

BATTERY Light and compact batteries have been adopted.
Item | 44B20L <Vehicles for Hong Kong spec.> | 75D23L <Vehicles for General Export (except for Hong Kong spec.), GCC, Australia and New zealand (2400)> <Option for Hong Kong spec.>
Voltage V | 12 | 12
Capacity (5-hour rate Ah) | 53 | 34
Electrolytic fluid specific gravity (fully charged state at 20°C) | 1.280 | 1.280

[54A] CHASSIS ELECTRICAL - - BATTERY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation