[52A] INTERIOR - - HEADLINING - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

HEADLINING

REMOVAL AND INSTALLATION
Pre-removal and Post-installation Operation Removal and Installation of Front Pillar Trim, Centre Pillar Trim Upper, Quarter Trim Upper (Refer to ).
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Assist grip
|  | 2. | Rear room lamp assembly
|  | 3. | Map lamp and front room lamp assembly
|  | 4. | Sunroof switch cover <Vehicle with sunroof>
<<A>> |  | 5. | Sun visor holder
|  | 6. | Sun visor assembly
|  | 7. | Front roof rail edge trim <Vehicles with sunroof>
|  | 8. | Rear roof rail edge trim <Vehicles with sunroof (Hong Kong)>
|  | 9. | Headlining
|  | 10. | Roof bracket <Vehicles with sunroof (except for Hong Kong)>
|  | 11. | Front side roof rib <Except vehicles for Hong Kong>
|  | 12. | Rear side roof rib <Except vehicles for Hong Kong>
| REMOVAL SERVICE POINT
| <<A>> SUN VISOR HOLDER REMOVAL
| Insert the special tool ornament remover (MB990784) into side claws of the sun visor holder through the both sides to remove the hinges.

[52A] INTERIOR - - HEADLINING - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation