[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS> - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 3: The ignition key is at the LOCK (OFF) position, but the selector lever can be moved from the P to the R position when the brake pedal is depressed. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 3: The ignition key is at the LOCK (OFF) position, but the selector lever can be moved from the P to the R position when the brake pedal is depressed.
COMMENTS ON TROUBLE SYMPTOM The cause is probably a malfunction of the key interlock cable or ignition key cylinder lock bar.
Possible causes Malfunction of key interlock cable Malfunction of lock bar
DIAGNOSIS Check by referring to the possible causes.

[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS> - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 3: The ignition key is at the LOCK (OFF) position, but the selector lever can be moved from the P to the R position when the brake pedal is depressed. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation